\hypertarget{ata-micron_8c}{}\doxysection{dev/ata/chipsets/ata-\/micron.c File Reference}
\label{ata-micron_8c}\index{dev/ata/chipsets/ata-\/micron.c@{dev/ata/chipsets/ata-\/micron.c}}
{\ttfamily \#include $<$sys/cdefs.\+h$>$}\newline
{\ttfamily \#include $<$sys/param.\+h$>$}\newline
{\ttfamily \#include $<$sys/module.\+h$>$}\newline
{\ttfamily \#include $<$sys/systm.\+h$>$}\newline
{\ttfamily \#include $<$sys/kernel.\+h$>$}\newline
{\ttfamily \#include $<$sys/ata.\+h$>$}\newline
{\ttfamily \#include $<$sys/bus.\+h$>$}\newline
{\ttfamily \#include $<$sys/endian.\+h$>$}\newline
{\ttfamily \#include $<$sys/malloc.\+h$>$}\newline
{\ttfamily \#include $<$sys/lock.\+h$>$}\newline
{\ttfamily \#include $<$sys/mutex.\+h$>$}\newline
{\ttfamily \#include $<$sys/sema.\+h$>$}\newline
{\ttfamily \#include $<$sys/taskqueue.\+h$>$}\newline
{\ttfamily \#include $<$vm/uma.\+h$>$}\newline
{\ttfamily \#include $<$machine/stdarg.\+h$>$}\newline
{\ttfamily \#include $<$machine/resource.\+h$>$}\newline
{\ttfamily \#include $<$machine/bus.\+h$>$}\newline
{\ttfamily \#include $<$sys/rman.\+h$>$}\newline
{\ttfamily \#include $<$dev/pci/pcivar.\+h$>$}\newline
{\ttfamily \#include $<$dev/pci/pcireg.\+h$>$}\newline
{\ttfamily \#include $<$dev/ata/ata-\/all.\+h$>$}\newline
{\ttfamily \#include $<$dev/ata/ata-\/pci.\+h$>$}\newline
{\ttfamily \#include $<$ata\+\_\+if.\+h$>$}\newline
Include dependency graph for ata-\/micron.c\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{d2/d96/ata-micron_8c__incl}
\end{center}
\end{figure}
\doxysubsection*{Functions}
\begin{DoxyCompactItemize}
\item 
\mbox{\hyperlink{ata-micron_8c_a8c3ef283470a68cd30afe9b8a72cb60f}{\+\_\+\+\_\+\+FBSDID}} (\char`\"{}\$Free\+BSD\$\char`\"{})
\item 
static int \mbox{\hyperlink{ata-micron_8c_a347a6478cb7e5af3862208ff84501c42}{ata\+\_\+micron\+\_\+probe}} (device\+\_\+t dev)
\item 
\mbox{\hyperlink{ata-micron_8c_adcba2d6b99c09fb8964e6a46a9cde98b}{ATA\+\_\+\+DECLARE\+\_\+\+DRIVER}} (ata\+\_\+micron)
\end{DoxyCompactItemize}


\doxysubsection{Function Documentation}
\mbox{\Hypertarget{ata-micron_8c_a8c3ef283470a68cd30afe9b8a72cb60f}\label{ata-micron_8c_a8c3ef283470a68cd30afe9b8a72cb60f}} 
\index{ata-\/micron.c@{ata-\/micron.c}!\_\_FBSDID@{\_\_FBSDID}}
\index{\_\_FBSDID@{\_\_FBSDID}!ata-\/micron.c@{ata-\/micron.c}}
\doxysubsubsection{\texorpdfstring{\_\_FBSDID()}{\_\_FBSDID()}}
{\footnotesize\ttfamily \+\_\+\+\_\+\+FBSDID (\begin{DoxyParamCaption}\item[{\char`\"{}\$Free\+BSD\$\char`\"{}}]{ }\end{DoxyParamCaption})}

\mbox{\Hypertarget{ata-micron_8c_adcba2d6b99c09fb8964e6a46a9cde98b}\label{ata-micron_8c_adcba2d6b99c09fb8964e6a46a9cde98b}} 
\index{ata-\/micron.c@{ata-\/micron.c}!ATA\_DECLARE\_DRIVER@{ATA\_DECLARE\_DRIVER}}
\index{ATA\_DECLARE\_DRIVER@{ATA\_DECLARE\_DRIVER}!ata-\/micron.c@{ata-\/micron.c}}
\doxysubsubsection{\texorpdfstring{ATA\_DECLARE\_DRIVER()}{ATA\_DECLARE\_DRIVER()}}
{\footnotesize\ttfamily ATA\+\_\+\+DECLARE\+\_\+\+DRIVER (\begin{DoxyParamCaption}\item[{ata\+\_\+micron}]{ }\end{DoxyParamCaption})}

\mbox{\Hypertarget{ata-micron_8c_a347a6478cb7e5af3862208ff84501c42}\label{ata-micron_8c_a347a6478cb7e5af3862208ff84501c42}} 
\index{ata-\/micron.c@{ata-\/micron.c}!ata\_micron\_probe@{ata\_micron\_probe}}
\index{ata\_micron\_probe@{ata\_micron\_probe}!ata-\/micron.c@{ata-\/micron.c}}
\doxysubsubsection{\texorpdfstring{ata\_micron\_probe()}{ata\_micron\_probe()}}
{\footnotesize\ttfamily static int ata\+\_\+micron\+\_\+probe (\begin{DoxyParamCaption}\item[{device\+\_\+t}]{dev }\end{DoxyParamCaption})\hspace{0.3cm}{\ttfamily [static]}}



Definition at line \mbox{\hyperlink{ata-micron_8c_source_l00059}{59}} of file \mbox{\hyperlink{ata-micron_8c_source}{ata-\/micron.\+c}}.



References \mbox{\hyperlink{ata-pci_8c_source_l00382}{ata\+\_\+generic\+\_\+chipinit()}}, \mbox{\hyperlink{ata-pci_8h_source_l00274}{ATA\+\_\+\+MICRON\+\_\+\+RZ1000}}, \mbox{\hyperlink{ata-pci_8h_source_l00275}{ATA\+\_\+\+MICRON\+\_\+\+RZ1001}}, \mbox{\hyperlink{ata-pci_8h_source_l00059}{ata\+\_\+pci\+\_\+controller\+::chipinit}}, and \mbox{\hyperlink{ata-pci_8h_source_l00045}{ata\+\_\+pci\+\_\+controller\+::dev}}.

Here is the call graph for this function\+:
\nopagebreak
\begin{figure}[H]
\begin{center}
\leavevmode
\includegraphics[width=350pt]{d8/d71/ata-micron_8c_a347a6478cb7e5af3862208ff84501c42_cgraph}
\end{center}
\end{figure}
