  % Handle batch mode
  % to overcome problems with too many open files
  \let\mypdfximage\pdfximage\def\pdfximage{\immediate\mypdfximage}
  % Set document class depending on configuration
  \documentclass[twoside]{book}
  %% moved from doxygen.sty due to workaround for LaTex 2019 version and unmaintained tabu package
  \usepackage{ifthen}
  \ifx\requestedLaTeXdate\undefined
    \usepackage{array}
  \else
    \usepackage{array}[=2016-10-06]
  \fi
  %%
  % Packages required by doxygen
  \usepackage{fixltx2e} % for \textsubscript
  \usepackage{doxygen}
  \usepackage{graphicx}
  \usepackage[utf8]{inputenc}
  \usepackage{makeidx}
  \PassOptionsToPackage{warn}{textcomp}
  \usepackage{textcomp}
  \usepackage[nointegrals]{wasysym}
  \usepackage{ifxetex}
  % NLS support packages
  % Define default fonts
  % Font selection
  \usepackage[T1]{fontenc}
  % set main and monospaced font
  \usepackage[scaled=.90]{helvet}
\usepackage{courier}
\renewcommand{\familydefault}{\sfdefault}
  \usepackage{sectsty}
  \allsectionsfont{%
    \fontseries{bc}\selectfont%
    \color{darkgray}%
  }
  \renewcommand{\DoxyLabelFont}{%
    \fontseries{bc}\selectfont%
    \color{darkgray}%
  }
  \newcommand{\+}{\discretionary{\mbox{\scriptsize$\hookleftarrow$}}{}{}}
   % Arguments of doxygenemoji:
   % 1) ':<text>:' form of the emoji, already LaTeX-escaped
   % 2) file with the name of the emoji without the .png extension
   % in case image exist use this otherwise use the ':<text>:' form
   \newcommand{\doxygenemoji}[2]{%
     \IfFileExists{./#2.png}{\raisebox{-0.1em}{\includegraphics[height=0.9em]{./#2.png}}}{#1}%
   }
  % Page & text layout
  \usepackage{geometry}
  \geometry{%
    a4paper,%
    top=2.5cm,%
    bottom=2.5cm,%
    left=2.5cm,%
    right=2.5cm%
  }
  % Allow a bit of overflow to go unnoticed by other means
  \tolerance=750
  \hfuzz=15pt
  \hbadness=750
  \setlength{\emergencystretch}{15pt}
  \setlength{\parindent}{0cm}
  \newcommand{\doxynormalparskip}{\setlength{\parskip}{3ex plus 2ex minus 2ex}}
  \newcommand{\doxytocparskip}{\setlength{\parskip}{1ex plus 0ex minus 0ex}}
  \doxynormalparskip
  % Redefine paragraph/subparagraph environments, using sectsty fonts
  \makeatletter
  \renewcommand{\paragraph}{%
    \@startsection{paragraph}{4}{0ex}{-1.0ex}{1.0ex}{%
      \normalfont\normalsize\bfseries\SS@parafont%
    }%
  }
  \renewcommand{\subparagraph}{%
    \@startsection{subparagraph}{5}{0ex}{-1.0ex}{1.0ex}{%
      \normalfont\normalsize\bfseries\SS@subparafont%
    }%
  }
  \makeatother
  \makeatletter
  \newcommand\hrulefilll{\leavevmode\leaders\hrule\hskip 0pt plus 1filll\kern\z@}
  \makeatother
  % Headers & footers
  \usepackage{fancyhdr}
  \pagestyle{fancyplain}
  \renewcommand{\footrulewidth}{0.4pt}
  \fancypagestyle{fancyplain}{
    \fancyhf{}
    \fancyhead[LE, RO]{\bfseries\thepage}
    \fancyhead[LO]{\bfseries\rightmark}
    \fancyhead[RE]{\bfseries\leftmark}
    \fancyfoot[LO, RE]{\bfseries\scriptsize Generated by Doxygen }
  }
  \fancypagestyle{plain}{
    \fancyhf{}
    \fancyfoot[LO, RE]{\bfseries\scriptsize Generated by Doxygen }
    \renewcommand{\headrulewidth}{0pt}
  }
  \pagestyle{fancyplain}
  \renewcommand{\chaptermark}[1]{%
    \markboth{#1}{}%
  }
  \renewcommand{\sectionmark}[1]{%
    \markright{\thesection\ #1}%
  }
  % ToC, LoF, LoT, bibliography, and index
  % Indices & bibliography
  \usepackage{natbib}
  \usepackage[titles]{tocloft}
  \setcounter{tocdepth}{3}
  \setcounter{secnumdepth}{5}
  % creating indexes
  \makeindex
  \usepackage{newunicodechar}
  \newunicodechar{⁻}{${}^{-}$}% Superscript minus
  \newunicodechar{²}{${}^{2}$}% Superscript two
  \newunicodechar{³}{${}^{3}$}% Superscript three
  % Hyperlinks
    % Hyperlinks (required, but should be loaded last)
    \ifpdf
      \usepackage[pdftex,pagebackref=true]{hyperref}
    \else
      \ifxetex
        \usepackage[pagebackref=true]{hyperref}
      \else
        \usepackage[ps2pdf,pagebackref=true]{hyperref}
      \fi
    \fi
    \hypersetup{%
      colorlinks=true,%
      linkcolor=blue,%
      citecolor=blue,%
      unicode,%
      pdftitle=Free\+BSD kernel usb device Code,%
      pdfsubject=%
    }
  % Custom commands used by the header
  % Custom commands
  \newcommand{\clearemptydoublepage}{%
    \newpage{\pagestyle{empty}\cleardoublepage}%
  }
  % caption style definition
  \usepackage{caption}
  \captionsetup{labelsep=space,justification=centering,font={bf},singlelinecheck=off,skip=4pt,position=top}
  % in page table of contents
  \usepackage{etoc}
  \etocsettocstyle{\doxytocparskip}{\doxynormalparskip}
  % prevent numbers overlap the titles in toc
  \renewcommand{\numberline}[1]{#1~}
% End of preamble, now comes the document contents
%===== C O N T E N T S =====
\begin{document}
  \raggedbottom
  % Titlepage & ToC
    % To avoid duplicate page anchors due to reuse of same numbers for
    % the index (be it as roman numbers)
    \hypersetup{pageanchor=false,
                bookmarksnumbered=true,
                pdfencoding=unicode
               }
  \pagenumbering{alph}
  \begin{titlepage}
  \vspace*{7cm}
  \begin{center}%
  {\Large Free\+BSD kernel usb device Code}\\
  \vspace*{1cm}
  {\large Generated by Doxygen 1.9.3}\\
  \end{center}
  \end{titlepage}
  \clearemptydoublepage
  \pagenumbering{roman}
  \tableofcontents
  \clearemptydoublepage
  \pagenumbering{arabic}
  % re-enable anchors again
  \hypersetup{pageanchor=true}
%--- Begin generated contents ---
\chapter{Free\+BSD kernel usb device Code}
\label{index}\hypertarget{index}{}\input{index}
\chapter{Data Structure Index}
\input{annotated}
\chapter{File Index}
\input{files}
\chapter{Data Structure Documentation}
\input{d3/d3c/struct____packed}
\input{dc/df7/structacpi__uhub__port}
\input{d7/d7e/structacpi__uhub__softc}
\input{dc/d5c/structatmegadci__config__desc}
\input{df/dc5/structatmegadci__flags}
\input{d4/d0c/unionatmegadci__hub__temp}
\input{dc/d58/structatmegadci__softc}
\input{da/dd9/structatmegadci__std__temp}
\input{de/d50/structatmegadci__td}
\input{d2/d26/structatp__softc}
\input{d1/df7/structatp__stroke}
\input{d3/d16/structaue__intrpkt}
\input{d8/d36/structaue__rxpkt}
\input{d6/d05/structaue__softc}
\input{df/dbd/structavr32dci__config__desc}
\input{db/d69/structavr32dci__flags}
\input{d5/d64/unionavr32dci__hub__temp}
\input{d7/da5/structavr32dci__softc}
\input{d4/d2e/structavr32dci__std__temp}
\input{d8/dd4/structavr32dci__td}
\input{d3/d36/structawusbdrd__softc}
\input{d7/d43/structax88772b__mfb}
\input{da/dae/structaxe__csum__hdr}
\input{df/d85/structaxe__sframe__hdr}
\input{d6/d46/structaxe__softc}
\input{df/dea/structaxge__frame__rxhdr}
\input{db/d3d/structaxge__frame__txhdr}
\input{db/d51/structaxge__softc}
\input{da/d15/structbbb__cbw}
\input{d5/d13/structbbb__csw}
\input{d7/d72/structbbb__transfer}
\input{d4/d77/structbt__data}
\input{d6/db5/structcdce__ncm}
\input{d9/d28/structcdce__softc}
\input{dd/d9c/structcdceem__softc}
\input{d2/d5e/structcfumass__cbw__t}
\input{d6/dd6/structcfumass__csw__t}
\input{d6/d91/structcfumass__softc}
\input{d2/d7f/structclk__list}
\input{df/df2/structcp2112__softc}
\input{d1/d62/structcp2112gpio__softc}
\input{d9/dcc/structcp2112iic__softc}
\input{d0/d3e/structcue__softc}
\input{d4/d62/structdwc__otg__chan__state}
\input{d9/d82/structdwc__otg__config__desc}
\input{d9/de8/structdwc__otg__fdt__softc}
\input{d8/d30/structdwc__otg__flags}
\input{d9/d8f/uniondwc__otg__hub__temp}
\input{da/df5/structdwc__otg__profile}
\input{d3/d31/structdwc__otg__softc}
\input{d5/d23/structdwc__otg__std__temp}
\input{d1/d5e/structdwc__otg__td}
\input{da/d6f/structdwc__otg__tt__info}
\input{d8/d69/structehci__config__desc}
\input{db/d53/structehci__fstn}
\input{dc/d77/unionehci__hub__desc}
\input{df/d14/structehci__hw__softc}
\input{d7/d12/structehci__itd}
\input{d5/d51/structehci__msm__softc}
\input{d1/dc0/structehci__qh}
\input{d4/d8d/structehci__qh__sub}
\input{d6/d5a/structehci__qtd}
\input{d3/da3/structehci__sitd}
\input{db/d7f/structehci__softc}
\input{df/dec/structehci__std__temp}
\input{d9/dfc/structfg__dev__params}
\input{d9/d00/structfg__pspan}
\input{da/daf/structfg__stroke__component}
\input{d3/d12/structg__audio__softc}
\input{d0/d94/structg__keyboard__data}
\input{d2/d00/structg__keyboard__softc}
\input{dc/d26/structg__modem__softc}
\input{d7/d9f/structg__mouse__data}
\input{d4/d2a/structg__mouse__softc}
\input{de/d36/structgeneric__ehci__fdt__softc}
\input{da/ddc/structgeneric__ohci__softc}
\input{d3/db8/structgpio__config__req}
\input{d2/d37/structgpio__get__req}
\input{da/deb/structgpio__set__req}
\input{d4/dad/structhub__result}
\input{d4/d43/structhwrst__list}
\input{d3/dd8/structi2c__cfg__req}
\input{dd/d9d/structi2c__data__read__force__send__req}
\input{dc/dc1/structi2c__data__read__resp}
\input{dc/d1f/structi2c__read__req}
\input{d9/d97/structi2c__write__read__req}
\input{d3/d25/structi2c__write__req}
\input{d6/d86/structi2c__xfer__status__req}
\input{d0/d63/structi2c__xfer__status__resp}
\input{de/d24/structimx__ehci__softc}
\input{d8/d16/structimx__usbmisc__softc}
\input{db/d58/structipheth__softc}
\input{d8/d7a/structjtag__by__name}
\input{d1/dcd/structkue__ether__desc}
\input{d3/d34/structkue__softc}
\input{d2/d6d/structmos__softc}
\input{d4/d85/structmuge__softc}
\input{d2/d35/structmusb__otg__ep__cfg}
\input{d3/d2a/structmusbotg__config__desc}
\input{d0/d3d/structmusbotg__dma}
\input{d2/d4b/structmusbotg__flags}
\input{dc/d79/unionmusbotg__hub__temp}
\input{db/d90/structmusbotg__softc}
\input{d5/de3/structmusbotg__std__temp}
\input{da/df9/structmusbotg__td}
\input{d3/d80/structndis__802__11__configuration}
\input{d0/d3f/structndis__802__11__configuration__fh}
\input{dc/d6c/structndis__802__11__fixed__ies}
\input{da/d22/structndis__802__11__ssid}
\input{de/d73/structndis__wlan__bssid__ex}
\input{d5/da4/structngudbpstat}
\input{d7/d85/structohci__config__desc}
\input{d6/d17/structohci__ed}
\input{db/d69/structohci__hcca}
\input{d8/daa/unionohci__hub__desc}
\input{d9/d44/structohci__hw__softc}
\input{de/dbb/structohci__itd}
\input{d4/d4a/structohci__softc}
\input{da/d7c/structohci__std__temp}
\input{de/db8/structohci__td}
\input{d6/daa/structphy__list}
\input{db/d2c/structr92s__add__ba__event}
\input{d9/da6/structr92s__add__ba__req}
\input{df/d64/structr92s__event__join__bss}
\input{da/dbb/structr92s__fw__cmd__auth}
\input{d0/dff/structr92s__fw__cmd__hdr}
\input{d0/d23/structr92s__fw__cmd__set__key}
\input{d2/d1d/structr92s__fw__cmd__set__key__mac}
\input{d0/da7/structr92s__fw__cmd__sitesurvey}
\input{db/dd9/structr92s__fw__hdr}
\input{d9/d11/structr92s__fw__priv}
\input{d5/db5/structr92s__pwr__cmd}
\input{d8/d79/structr92s__rx__cck}
\input{d3/db7/structr92s__rx__phystat}
\input{db/d79/structr92s__rx__stat}
\input{dd/d7b/structr92s__set__channel}
\input{dd/d45/structr92s__set__pwr__mode}
\input{d9/d1e/structr92s__tx__desc}
\input{d5/d12/structrfprog}
\input{d2/d3c/structRioCommand}
\input{df/d60/structrsu__data}
\input{df/d32/structrsu__rx__radiotap__header}
\input{de/d03/structrsu__softc}
\input{d1/d19/structrsu__tx__radiotap__header}
\input{d2/d0c/structrsu__vap}
\input{db/de5/structrt2860__rate}
\input{da/ddf/structrt2860__rxd}
\input{d8/d63/structrt2860__rxwi}
\input{d1/df6/structrt2860__txd}
\input{d2/d94/structrt2860__txwi}
\input{d6/d28/structrt2870__rxd}
\input{d0/d51/structrt2870__txd}
\input{df/d5d/structrt5592__freqs}
\input{d7/d71/structrue__intrpkt}
\input{db/d59/structrue__softc}
\input{d8/d82/structrum__cmdq}
\input{df/d50/structrum__rx__desc}
\input{d8/d44/structrum__rx__radiotap__header}
\input{d7/d4f/structrum__softc}
\input{d3/df0/structrum__tx__data}
\input{da/d05/structrum__tx__desc}
\input{d0/d4b/structrum__tx__radiotap__header}
\input{da/df0/structrum__vap}
\input{d4/d23/structrun__cmdq}
\input{d8/d72/structrun__endpoint__queue}
\input{d8/df4/structrun__node}
\input{d1/d7b/structrun__rx__radiotap__header}
\input{dd/d59/structrun__softc}
\input{de/d41/unionrun__stats}
\input{de/dd5/structrun__tx__data}
\input{df/dac/structrun__tx__radiotap__header}
\input{d0/d39/structrun__vap}
\input{db/d00/unionsec__param}
\input{d3/d7d/structsmsc__softc}
\input{da/d87/structsnps__dwc3__softc}
\input{d4/d1e/structtp__finger}
\input{da/d7d/structtp__header}
\input{d1/dbf/structu3g__softc}
\input{df/dfa/structuark__softc}
\input{dc/de0/structuath__chunk}
\input{d2/d5b/structuath__cmd}
\input{de/d4d/structuath__cmd__0c}
\input{d4/d61/structuath__cmd__31}
\input{d9/dbf/structuath__cmd__assoc__bss}
\input{d7/de8/structuath__cmd__bind}
\input{da/dc1/structuath__cmd__connection__attr}
\input{d1/d57/structuath__cmd__create__connection}
\input{d1/db3/structuath__cmd__crypto}
\input{d7/d07/structuath__cmd__hdr}
\input{d4/d37/structuath__cmd__host__available}
\input{d7/de2/structuath__cmd__join__bss}
\input{da/d3b/structuath__cmd__ledblink}
\input{d8/de2/structuath__cmd__ledstate}
\input{d4/d12/structuath__cmd__ledsteady}
\input{d5/d47/structuath__cmd__rates}
\input{d0/dd0/structuath__cmd__rateset}
\input{d5/d1e/structuath__cmd__reset}
\input{d4/dc5/structuath__cmd__rx__filter}
\input{d0/dbf/structuath__cmd__rx__mcast__filter}
\input{db/df1/structuath__cmd__set__associd}
\input{d5/d3a/structuath__cmd__set__stabeacon__timers}
\input{d9/d4b/structuath__cmd__start__bss}
\input{d4/dba/structuath__cmd__stoptxdma}
\input{d0/d45/structuath__cmd__txq__attr}
\input{d3/d10/structuath__cmd__txq__setparams}
\input{d3/d8d/structuath__cmd__txq__setup}
\input{d7/d46/structuath__cmd__update__bss__attribute}
\input{d1/d74/structuath__cmd__update__bss__attribute__key}
\input{d4/d1a/structuath__connkey__rec}
\input{d4/dae/structuath__data}
\input{df/dca/structuath__devcap}
\input{d7/daf/structuath__fwblock}
\input{d5/d4d/structuath__read__mac}
\input{dc/d22/structuath__rx__desc}
\input{de/d74/structuath__rx__radiotap__header}
\input{d2/ddb/structuath__softc}
\input{da/db7/structuath__stat}
\input{d2/db2/structuath__tx__desc}
\input{da/dd2/structuath__tx__radiotap__header}
\input{d8/dec/structuath__vap}
\input{d6/d11/structuath__wme__settings}
\input{da/de9/structuath__write__mac}
\input{d9/dfe/structubsa__softc}
\input{d7/d25/structubser__softc}
\input{d7/d10/structuchcom__divider}
\input{d4/d04/structuchcom__divider__record}
\input{d2/d28/structuchcom__softc}
\input{d4/d52/structucom__callback}
\input{d4/db7/structucom__cfg__task}
\input{d2/d89/structucom__param__task}
\input{d0/de9/structucom__softc}
\input{d5/d72/structucom__super__softc}
\input{db/d71/structucycom__softc}
\input{da/d24/structudav__rxpkt}
\input{da/d6b/structudav__softc}
\input{da/d58/structudbp__softc}
\input{d0/ddc/structudl__buffer}
\input{dd/d84/structudl__cmd__buf}
\input{d1/d66/structudl__mode}
\input{df/df8/structudl__softc}
\input{dc/dbc/structuep__softc}
\input{dd/d9c/structufoma__mobile__acm__descriptor}
\input{d0/d45/structufoma__softc}
\input{d6/dcc/structuftdi__bitmode}
\input{d2/d37/structuftdi__eeio}
\input{dd/d0e/structuftdi__param__config}
\input{de/d7f/structuftdi__softc}
\input{dc/d36/structugensa__softc}
\input{d4/d62/structugensa__sub__softc}
\input{de/d3d/structugold__readout__msg}
\input{d5/d57/structugold__softc}
\input{d0/de4/structuhci__config__desc}
\input{d9/d85/unionuhci__hub__desc}
\input{d0/d83/structuhci__hw__softc}
\input{db/ddf/structuhci__mem__layout}
\input{d1/dce/structuhci__qh}
\input{d2/db0/structuhci__softc}
\input{dc/d12/structuhci__std__temp}
\input{d7/d37/structuhci__td}
\input{dc/d1e/structuhid__snes__softc}
\input{dc/dd3/structuhid__softc}
\input{d1/deb/structuhso__softc}
\input{d4/db6/structuhso__tty}
\input{d4/d4c/structuhub__current__state}
\input{d8/df6/structuhub__softc}
\input{d6/d7b/structuipaq__softc}
\input{d8/d58/structukbd__data}
\input{d5/de6/structukbd__softc}
\input{d2/d66/structuled__color}
\input{d8/def/structuled__softc}
\input{d9/d4f/structulpt__softc}
\input{de/d7f/structumass__probe__proto}
\input{dc/d91/structumass__softc}
\input{db/d2c/structumcpc__modetostr__tab}
\input{dd/d80/structumcs7840__port__registers}
\input{d6/d0b/structumcs7840__softc}
\input{d7/d91/structumcs7840__softc__oneport}
\input{db/d95/structumct__softc}
\input{df/d46/structumodem__softc}
\input{d7/dd4/structumoscom__softc}
\input{d1/d00/structums__info}
\input{da/dab/structums__softc}
\input{dd/de9/structupgt__data}
\input{d2/d17/structupgt__eeprom__freq3__header}
\input{db/df1/structupgt__eeprom__freq4__1}
\input{d3/d56/structupgt__eeprom__freq4__2}
\input{d3/d80/structupgt__eeprom__freq4__header}
\input{d5/db6/structupgt__eeprom__header}
\input{d5/dae/structupgt__eeprom__option}
\input{d1/ddb/structupgt__eeprom__option__hwrx}
\input{dd/d3b/structupgt__fw__bra__descr}
\input{d9/dfd/structupgt__fw__bra__option}
\input{d7/deb/structupgt__fw__x2__header}
\input{d0/d95/structupgt__lmac__channel}
\input{d2/d73/structupgt__lmac__eeprom}
\input{d4/da7/structupgt__lmac__filter}
\input{dc/dcd/structupgt__lmac__freq3}
\input{d5/d9b/structupgt__lmac__freq4}
\input{d9/d1c/structupgt__lmac__freq6}
\input{df/d02/structupgt__lmac__h1}
\input{d5/d32/structupgt__lmac__h2}
\input{d9/d0f/structupgt__lmac__header}
\input{d1/da9/structupgt__lmac__led}
\input{dc/da9/structupgt__lmac__mem}
\input{d8/d4c/structupgt__lmac__rx__desc}
\input{dc/d48/structupgt__lmac__stats}
\input{d3/df6/structupgt__lmac__tx__desc}
\input{dc/d51/structupgt__lmac__tx__desc__wep}
\input{d0/dec/structupgt__lmac__tx__done__desc}
\input{df/d80/structupgt__memory}
\input{d8/d37/structupgt__memory__page}
\input{d2/dfb/structupgt__rx__radiotap__header}
\input{dd/d71/structupgt__softc}
\input{d7/d47/structupgt__stat}
\input{de/dd2/structupgt__tx__radiotap__header}
\input{d7/d17/structupgt__vap}
\input{d8/d9e/structuplcom__softc}
\input{d3/dee/structural__rx__desc}
\input{d6/d24/structural__rx__radiotap__header}
\input{df/d62/structural__softc}
\input{db/d70/structural__tx__data}
\input{d3/dd7/structural__tx__desc}
\input{d5/df2/structural__tx__radiotap__header}
\input{dd/d79/structural__vap}
\input{d0/df8/structure__intrpkt}
\input{dc/dcc/structure__rxpkt}
\input{d2/d7f/structure__softc}
\input{d4/df8/structure__txpkt}
\input{d9/dcf/structurio__softc}
\input{d7/dd9/structurndis__softc}
\input{d0/d28/structurtw__8187b__rxhdr}
\input{dc/db2/structurtw__8187b__txhdr}
\input{d1/d8f/structurtw__8187l__rxhdr}
\input{d1/d97/structurtw__8187l__txhdr}
\input{d9/d40/structurtw__data}
\input{da/d7e/structurtw__pair}
\input{df/d25/structurtw__rx__radiotap__header}
\input{da/db7/structurtw__softc}
\input{df/d26/structurtw__stats}
\input{de/dcd/structurtw__tx__radiotap__header}
\input{d2/df4/structurtw__vap}
\input{d4/d13/structusb__alt__interface}
\input{d3/dd8/structusb__attach__arg}
\input{de/d36/structusb__bos__cap__descriptor}
\input{dd/d05/structusb__bos__descriptor}
\input{de/dd0/structusb__bus}
\input{dc/dfe/structusb__bus__methods}
\input{d8/da3/structusb__bus__msg}
\input{da/db7/structusb__callout}
\input{dc/d39/structusb__cdc__abstract__state}
\input{d8/da7/structusb__cdc__acm__descriptor}
\input{d6/d07/structusb__cdc__cm__descriptor}
\input{d2/d6f/structusb__cdc__ethernet__descriptor}
\input{d1/da3/structusb__cdc__header__descriptor}
\input{d2/d08/structusb__cdc__line__state}
\input{d4/d2f/structusb__cdc__notification}
\input{de/d24/structusb__cdc__union__descriptor}
\input{d2/d2c/structusb__cdev__privdata}
\input{de/dba/structusb__cdev__refdata}
\input{d2/d24/structusb__config}
\input{d1/d25/structusb__config__descriptor}
\input{d8/dd2/structusb__ctl__request}
\input{df/da5/structusb__descriptor}
\input{df/de6/structusb__devcap__container__id__descriptor}
\input{da/d11/structusb__devcap__ss__descriptor}
\input{d4/d64/structusb__devcap__usb2ext__descriptor}
\input{d3/da1/structusb__device}
\input{d4/dfa/structusb__device__descriptor}
\input{d8/d46/structusb__device__flags}
\input{da/dea/structusb__device__id}
\input{d8/d0e/structusb__device__info}
\input{d0/ddc/structusb__device__port__path}
\input{d6/d1a/structusb__device__qualifier}
\input{d2/d08/structusb__device__request}
\input{df/d24/unionusb__device__scratch}
\input{d0/d09/structusb__device__statistics}
\input{de/d39/structusb__device__stats}
\input{d6/d0c/structusb__dma__parent__tag}
\input{de/d5a/structusb__dma__tag}
\input{d3/d18/structusb__done__msg}
\input{d0/dae/structusb__endpoint}
\input{d2/d50/structusb__endpoint__descriptor}
\input{d5/d2f/structusb__endpoint__ss__comp__descriptor}
\input{d1/d4b/structusb__ether}
\input{d0/d04/structusb__ether__cfg__task}
\input{df/d62/structusb__ether__methods}
\input{da/d49/structusb__fifo}
\input{dc/db1/structusb__fifo__methods}
\input{d7/d7c/structusb__fifo__sc}
\input{d7/dda/structusb__fs__clear__stall__sync}
\input{d6/dfc/structusb__fs__close}
\input{db/d43/structusb__fs__complete}
\input{d1/d26/structusb__fs__endpoint}
\input{d8/d5d/structusb__fs__init}
\input{da/db0/structusb__fs__open}
\input{da/d74/structusb__fs__open__stream}
\input{db/d00/structusb__fs__privdata}
\input{d7/d3c/structusb__fs__start}
\input{d9/dec/structusb__fs__stop}
\input{de/dcb/structusb__fs__uninit}
\input{da/d8f/structusb__gen__descriptor}
\input{d6/da0/structusb__gen__quirk}
\input{d5/de4/structusb__hid__descriptor}
\input{de/d98/structusb__host__endpoint}
\input{d9/d31/structusb__host__interface}
\input{d5/dde/structusb__hub}
\input{d4/d5a/structusb__hub__descriptor}
\input{da/da2/structusb__hub__descriptor__min}
\input{d2/de5/structusb__hub__ss__descriptor}
\input{d3/db7/structusb__hub__status}
\input{d9/d53/structusb__hw__ep__profile}
\input{dc/db4/structusb__hw__ep__scratch}
\input{d9/d52/structusb__hw__ep__scratch__sub}
\input{de/d3c/structusb__idesc__parse__state}
\input{d2/dba/structusb__ifqueue}
\input{da/d4b/structusb__interface}
\input{dd/de6/structusb__interface__assoc__descriptor}
\input{d4/dfc/structusb__interface__descriptor}
\input{d2/dfa/structusb__mbuf}
\input{d0/dc9/structusb__ncm16__dp}
\input{d2/d80/structusb__ncm16__dpt}
\input{d3/d37/structusb__ncm16__hdr}
\input{d3/dc5/structusb__ncm32__dp}
\input{dc/d79/structusb__ncm32__dpt}
\input{d0/d0e/structusb__ncm32__hdr}
\input{d0/d14/structusb__ncm__func__descriptor}
\input{d6/dc5/structusb__ncm__parameters}
\input{de/d4c/structusb__nop__xceiv__softc}
\input{d0/d5f/structusb__otg__descriptor}
\input{d1/d87/structusb__page}
\input{d2/dc1/structusb__page__cache}
\input{db/d08/structusb__page__search}
\input{dd/df9/structusb__pipe__methods}
\input{dc/dbf/structusb__port}
\input{d4/d57/structusb__port__status}
\input{d8/d31/structusb__power__save}
\input{d9/d53/structusb__proc__msg}
\input{d5/db4/structusb__process}
\input{df/d89/structusb__quirk__entry}
\input{d3/d40/structusb__read__dir}
\input{d7/dac/structusb__setup__params}
\input{d9/d80/structusb__status}
\input{da/de6/structusb__std__packet__size}
\input{d3/d12/structusb__string__descriptor}
\input{d2/d38/structusb__string__lang}
\input{da/d48/structusb__symlink}
\input{df/d78/structusb__temp__config__desc}
\input{da/d19/structusb__temp__data}
\input{d8/d94/structusb__temp__device__desc}
\input{d7/ddf/structusb__temp__endpoint__desc}
\input{d8/d6e/structusb__temp__interface__desc}
\input{d0/dde/structusb__temp__interval}
\input{d0/d8d/structusb__temp__packet__size}
\input{de/de8/structusb__temp__setup}
\input{d2/d14/structusb__udev__msg}
\input{d5/dc7/structusb__xfer}
\input{dc/dbc/structusb__xfer__flags}
\input{d1/ddb/structusb__xfer__flags__int}
\input{d8/d3d/structusb__xfer__queue}
\input{dc/d72/structusb__xfer__root}
\input{d2/dfb/structusbd__lookup__info}
\input{de/d8d/unionusbhid__device__request}
\input{da/dd9/structusbhid__softc}
\input{da/d98/structusbhid__xfer__ctx}
\input{de/d4b/structusbpf__framehdr}
\input{d9/dc0/structusbpf__pkthdr}
\input{da/d00/structusie__cns}
\input{df/d82/structusie__desc}
\input{db/dab/structusie__hip}
\input{d4/d52/structusie__lsi}
\input{d8/dff/structusie__net__info}
\input{dc/d6f/structusie__softc}
\input{de/db4/structuslcom__softc}
\input{d7/dbc/structuss820__flags}
\input{dc/d83/unionuss820__hub__temp}
\input{d0/d44/structuss820__std__temp}
\input{d5/d8d/structuss820dci__config__desc}
\input{d7/d7b/structuss820dci__softc}
\input{d1/dd0/structuss820dci__td}
\input{d2/de8/structustorage__fs__lun}
\input{da/d3d/structustorage__fs__softc}
\input{df/d3e/structuvisor__connection__info}
\input{d1/d66/structuvisor__palm__connection__info}
\input{d4/d25/structuvisor__softc}
\input{d8/d02/structuvscom__softc}
\input{d1/d61/structversion__request}
\input{db/d7e/structwmt__absinfo}
\input{d8/d76/structwmt__hid__map__item}
\input{db/dda/structwmt__softc}
\input{d9/d63/structwsp__dev__params}
\input{d1/d08/structwsp__finger}
\input{db/d5b/structwsp__finger__sensor__data}
\input{dc/d29/structwsp__param}
\input{d2/dff/structwsp__softc}
\input{d7/daf/structwsp__tp}
\input{dd/dd0/structwsp__tuning}
\input{d2/d05/structxhci__bos__desc}
\input{d6/d74/structxhci__command}
\input{d6/dab/structxhci__config__desc}
\input{da/db6/structxhci__dev__ctx}
\input{dc/dca/structxhci__dev__ctx64}
\input{d0/df2/structxhci__dev__ctx__addr}
\input{d8/d55/structxhci__dev__endpoint__trbs}
\input{dd/d91/structxhci__endp__ctx}
\input{d0/de6/structxhci__endp__ctx64}
\input{d9/dbb/structxhci__endpoint__ext}
\input{dd/d20/structxhci__event__ring__seg}
\input{d1/d55/unionxhci__hub__desc}
\input{d0/d9b/structxhci__hw__dev}
\input{d3/de4/structxhci__hw__root}
\input{d0/db3/structxhci__hw__softc}
\input{d5/dfd/structxhci__input__ctx}
\input{d7/d15/structxhci__input__ctx64}
\input{dc/d0f/structxhci__input__dev__ctx}
\input{d6/d92/structxhci__input__dev__ctx64}
\input{dc/d9b/structxhci__slot__ctx}
\input{d2/d61/structxhci__slot__ctx64}
\input{de/d66/structxhci__softc}
\input{d3/dfa/structxhci__std__temp}
\input{d5/dd0/structxhci__stream__ctx}
\input{d3/d67/structxhci__td}
\input{d8/dfa/structxhci__trb}
\input{d6/ded/structzyd__cmd}
\input{d6/dac/structzyd__mac__pair}
\input{dd/d05/structzyd__notif__retry}
\input{d9/d4f/structzyd__pair}
\input{d3/d70/structzyd__phy__pair}
\input{d6/d64/structzyd__plcphdr}
\input{d4/d33/structzyd__rf}
\input{d2/d98/structzyd__rfwrite__cmd}
\input{de/d99/structzyd__rq}
\input{d8/d74/structzyd__rx__data}
\input{df/d55/structzyd__rx__desc}
\input{d5/df3/structzyd__rx__radiotap__header}
\input{d8/d82/structzyd__rx__stat}
\input{d2/d2b/structzyd__softc}
\input{d4/d66/structzyd__tx__data}
\input{d4/de2/structzyd__tx__desc}
\input{d1/d89/structzyd__tx__radiotap__header}
\input{d4/dc7/structzyd__vap}
\chapter{File Documentation}
\input{d0/d69/atmegadci_8c}
\input{d0/d69/atmegadci_8c_source}
\input{d9/d19/atmegadci_8h}
\input{d9/d19/atmegadci_8h_source}
\input{d3/dbb/avr32dci_8c}
\input{d3/dbb/avr32dci_8c_source}
\input{de/dbf/avr32dci_8h}
\input{de/dbf/avr32dci_8h_source}
\input{d0/d0d/dwc3_8c}
\input{d0/d0d/dwc3_8c_source}
\input{d2/d1f/dwc3_8h}
\input{d2/d1f/dwc3_8h_source}
\input{d4/d4a/dwc__otg_8c}
\input{d4/d4a/dwc__otg_8c_source}
\input{d9/dc1/dwc__otg_8h}
\input{d9/dc1/dwc__otg_8h_source}
\input{dd/d84/dwc__otg__acpi_8c}
\input{dd/d84/dwc__otg__acpi_8c_source}
\input{d7/d9e/dwc__otg__fdt_8c}
\input{d7/d9e/dwc__otg__fdt_8c_source}
\input{de/d86/dwc__otg__fdt_8h}
\input{de/d86/dwc__otg__fdt_8h_source}
\input{d4/db4/dwc__otg__hisi_8c}
\input{d4/db4/dwc__otg__hisi_8c_source}
\input{dc/d06/dwc__otgreg_8h}
\input{dc/d06/dwc__otgreg_8h_source}
\input{d0/d24/ehci_8c}
\input{d0/d24/ehci_8c_source}
\input{d5/d69/ehci_8h}
\input{d5/d69/ehci_8h_source}
\input{d8/d43/ehci__fsl_8c}
\input{d8/d43/ehci__fsl_8c_source}
\input{d9/d28/ehci__imx_8c}
\input{d9/d28/ehci__imx_8c_source}
\input{d8/da1/ehci__msm_8c}
\input{d8/da1/ehci__msm_8c_source}
\input{dc/d16/ehci__mv_8c}
\input{dc/d16/ehci__mv_8c_source}
\input{db/d49/ehci__pci_8c}
\input{db/d49/ehci__pci_8c_source}
\input{d6/dbf/ehcireg_8h}
\input{d6/dbf/ehcireg_8h_source}
\input{de/d93/generic__ehci_8c}
\input{de/d93/generic__ehci_8c_source}
\input{df/d1d/generic__ehci_8h}
\input{df/d1d/generic__ehci_8h_source}
\input{d5/daf/generic__ehci__acpi_8c}
\input{d5/daf/generic__ehci__acpi_8c_source}
\input{d0/d59/generic__ehci__fdt_8c}
\input{d0/d59/generic__ehci__fdt_8c_source}
\input{d9/d82/generic__ohci_8c}
\input{d9/d82/generic__ohci_8c_source}
\input{db/de1/generic__usb__if_8m}
\input{db/de1/generic__usb__if_8m_source}
\input{d2/dfa/generic__xhci_8c}
\input{d2/dfa/generic__xhci_8c_source}
\input{d4/d87/generic__xhci_8h}
\input{d4/d87/generic__xhci_8h_source}
\input{d3/d51/generic__xhci__acpi_8c}
\input{d3/d51/generic__xhci__acpi_8c_source}
\input{da/d3d/generic__xhci__fdt_8c}
\input{da/d3d/generic__xhci__fdt_8c_source}
\input{d8/daa/musb__otg_8c}
\input{d8/daa/musb__otg_8c_source}
\input{db/d24/musb__otg_8h}
\input{db/d24/musb__otg_8h_source}
\input{df/d3f/musb__otg__allwinner_8c}
\input{df/d3f/musb__otg__allwinner_8c_source}
\input{d0/de5/ohci_8c}
\input{d0/de5/ohci_8c_source}
\input{dc/d61/ohci_8h}
\input{dc/d61/ohci_8h_source}
\input{df/dcc/ohci__pci_8c}
\input{df/dcc/ohci__pci_8c_source}
\input{de/dcd/ohcireg_8h}
\input{de/dcd/ohcireg_8h_source}
\input{d4/d5f/uhci_8c}
\input{d4/d5f/uhci_8c_source}
\input{dd/d51/uhci_8h}
\input{dd/d51/uhci_8h_source}
\input{d4/dd1/uhci__pci_8c}
\input{d4/dd1/uhci__pci_8c_source}
\input{d5/dfc/uhcireg_8h}
\input{d5/dfc/uhcireg_8h_source}
\input{d2/d22/usb__controller_8c}
\input{d2/d22/usb__controller_8c_source}
\input{d0/d32/usb__nop__xceiv_8c}
\input{d0/d32/usb__nop__xceiv_8c_source}
\input{df/d0b/uss820dci_8c}
\input{df/d0b/uss820dci_8c_source}
\input{d4/d20/uss820dci_8h}
\input{d4/d20/uss820dci_8h_source}
\input{d0/d15/xhci_8c}
\input{d0/d15/xhci_8c_source}
\input{d2/d28/xhci_8h}
\input{d2/d28/xhci_8h_source}
\input{df/d3f/xhci__pci_8c}
\input{df/d3f/xhci__pci_8c_source}
\input{d3/d8b/xhcireg_8h}
\input{d3/d8b/xhcireg_8h_source}
\input{d0/d2e/g__audio_8c}
\input{d0/d2e/g__audio_8c_source}
\input{d1/d63/g__audio_8h}
\input{d1/d63/g__audio_8h_source}
\input{d0/def/g__keyboard_8c}
\input{d0/def/g__keyboard_8c_source}
\input{dd/d9b/g__keyboard_8h}
\input{dd/d9b/g__keyboard_8h_source}
\input{de/d51/g__modem_8c}
\input{de/d51/g__modem_8c_source}
\input{d9/d2d/g__modem_8h}
\input{d9/d2d/g__modem_8h_source}
\input{db/dfd/g__mouse_8c}
\input{db/dfd/g__mouse_8c_source}
\input{d7/d17/g__mouse_8h}
\input{d7/d17/g__mouse_8h_source}
\input{d4/d9d/atp_8c}
\input{d4/d9d/atp_8c_source}
\input{df/dd8/uep_8c}
\input{df/dd8/uep_8c_source}
\input{d0/da2/uhid_8c}
\input{d0/da2/uhid_8c_source}
\input{db/d1e/uhid__snes_8c}
\input{db/d1e/uhid__snes_8c_source}
\input{da/d75/ukbd_8c}
\input{da/d75/ukbd_8c_source}
\input{de/d3c/ums_8c}
\input{de/d3c/ums_8c_source}
\input{d2/da3/usb__rdesc_8h}
\input{d2/da3/usb__rdesc_8h_source}
\input{da/d2b/usbhid_8c}
\input{da/d2b/usbhid_8c_source}
\input{de/d8d/wmt_8c}
\input{de/d8d/wmt_8c_source}
\input{d8/d0e/wsp_8c}
\input{d8/d0e/wsp_8c_source}
\input{df/d63/cp2112_8c}
\input{df/d63/cp2112_8c_source}
\input{dc/d7f/udbp_8c}
\input{dc/d7f/udbp_8c_source}
\input{de/dfe/udbp_8h}
\input{de/dfe/udbp_8h_source}
\input{d5/df4/ugold_8c}
\input{d5/df4/ugold_8c_source}
\input{df/d42/uled_8c}
\input{df/d42/uled_8c_source}
\input{d0/df7/if__aue_8c}
\input{d0/df7/if__aue_8c_source}
\input{d4/dde/if__auereg_8h}
\input{d4/dde/if__auereg_8h_source}
\input{dd/dc5/if__axe_8c}
\input{dd/dc5/if__axe_8c_source}
\input{d1/d13/if__axereg_8h}
\input{d1/d13/if__axereg_8h_source}
\input{df/d1e/if__axge_8c}
\input{df/d1e/if__axge_8c_source}
\input{d4/da4/if__axgereg_8h}
\input{d4/da4/if__axgereg_8h_source}
\input{d8/d63/if__cdce_8c}
\input{d8/d63/if__cdce_8c_source}
\input{d5/d48/if__cdceem_8c}
\input{d5/d48/if__cdceem_8c_source}
\input{d2/dda/if__cdcereg_8h}
\input{d2/dda/if__cdcereg_8h_source}
\input{d3/def/if__cue_8c}
\input{d3/def/if__cue_8c_source}
\input{d7/d19/if__cuereg_8h}
\input{d7/d19/if__cuereg_8h_source}
\input{d1/d15/if__ipheth_8c}
\input{d1/d15/if__ipheth_8c_source}
\input{d0/ddb/if__iphethvar_8h}
\input{d0/ddb/if__iphethvar_8h_source}
\input{d3/da5/if__kue_8c}
\input{d3/da5/if__kue_8c_source}
\input{d0/d49/if__kuefw_8h}
\input{d0/d49/if__kuefw_8h_source}
\input{d4/dd7/if__kuereg_8h}
\input{d4/dd7/if__kuereg_8h_source}
\input{d0/d46/if__mos_8c}
\input{d0/d46/if__mos_8c_source}
\input{df/ded/if__mosreg_8h}
\input{df/ded/if__mosreg_8h_source}
\input{d1/db3/if__muge_8c}
\input{d1/db3/if__muge_8c_source}
\input{d2/d97/if__mugereg_8h}
\input{d2/d97/if__mugereg_8h_source}
\input{d3/d60/if__rue_8c}
\input{d3/d60/if__rue_8c_source}
\input{de/d68/if__ruereg_8h}
\input{de/d68/if__ruereg_8h_source}
\input{d8/df6/if__smsc_8c}
\input{d8/df6/if__smsc_8c_source}
\input{d2/d20/if__smscreg_8h}
\input{d2/d20/if__smscreg_8h_source}
\input{de/dc0/if__udav_8c}
\input{de/dc0/if__udav_8c_source}
\input{d0/df7/if__udavreg_8h}
\input{d0/df7/if__udavreg_8h_source}
\input{da/df1/if__ure_8c}
\input{da/df1/if__ure_8c_source}
\input{d7/d79/if__urereg_8h}
\input{d7/d79/if__urereg_8h_source}
\input{d3/d73/if__urndis_8c}
\input{d3/d73/if__urndis_8c_source}
\input{d2/d63/if__urndisreg_8h}
\input{d2/d63/if__urndisreg_8h_source}
\input{d9/d2c/if__usie_8c}
\input{d9/d2c/if__usie_8c_source}
\input{df/d26/if__usievar_8h}
\input{df/d26/if__usievar_8h_source}
\input{d5/ddf/ruephy_8c}
\input{d5/ddf/ruephy_8c_source}
\input{d9/dc7/ruephyreg_8h}
\input{d9/dc7/ruephyreg_8h_source}
\input{df/dac/uhso_8c}
\input{df/dac/uhso_8c_source}
\input{d4/d76/usb__ethernet_8c}
\input{d4/d76/usb__ethernet_8c_source}
\input{d7/dfc/usb__ethernet_8h}
\input{d7/dfc/usb__ethernet_8h_source}
\input{d2/de0/usb__quirk_8c}
\input{d2/de0/usb__quirk_8c_source}
\input{d3/da0/usb__quirk_8h}
\input{d3/da0/usb__quirk_8h_source}
\input{d2/d62/u3g_8c}
\input{d2/d62/u3g_8c_source}
\input{df/d3c/uark_8c}
\input{df/d3c/uark_8c_source}
\input{d5/dab/ubsa_8c}
\input{d5/dab/ubsa_8c_source}
\input{d3/d42/ubser_8c}
\input{d3/d42/ubser_8c_source}
\input{d8/d33/uchcom_8c}
\input{d8/d33/uchcom_8c_source}
\input{df/dc2/ucycom_8c}
\input{df/dc2/ucycom_8c_source}
\input{d8/dde/ufoma_8c}
\input{d8/dde/ufoma_8c_source}
\input{d9/d95/uftdi_8c}
\input{d9/d95/uftdi_8c_source}
\input{df/da2/uftdi__reg_8h}
\input{df/da2/uftdi__reg_8h_source}
\input{da/dc8/ugensa_8c}
\input{da/dc8/ugensa_8c_source}
\input{df/d3d/uipaq_8c}
\input{df/d3d/uipaq_8c_source}
\input{d8/d9b/ulpt_8c}
\input{d8/d9b/ulpt_8c_source}
\input{d9/d02/umcs_8c}
\input{d9/d02/umcs_8c_source}
\input{d6/d75/umcs_8h}
\input{d6/d75/umcs_8h_source}
\input{d3/dfa/umct_8c}
\input{d3/dfa/umct_8c_source}
\input{d9/d44/umodem_8c}
\input{d9/d44/umodem_8c_source}
\input{d1/d23/umoscom_8c}
\input{d1/d23/umoscom_8c_source}
\input{d6/dfc/uplcom_8c}
\input{d6/dfc/uplcom_8c_source}
\input{df/dbe/usb__serial_8c}
\input{df/dbe/usb__serial_8c_source}
\input{de/dbd/usb__serial_8h}
\input{de/dbd/usb__serial_8h_source}
\input{d1/da6/uslcom_8c}
\input{d1/da6/uslcom_8c_source}
\input{dd/d11/uvisor_8c}
\input{dd/d11/uvisor_8c_source}
\input{d9/dc5/uvscom_8c}
\input{d9/dc5/uvscom_8c_source}
\input{d8/d8d/cfumass_8c}
\input{d8/d8d/cfumass_8c_source}
\input{d6/dec/rio500__usb_8h}
\input{d6/dec/rio500__usb_8h_source}
\input{d0/d34/umass_8c}
\input{d0/d34/umass_8c_source}
\input{dd/d25/urio_8c}
\input{dd/d25/urio_8c_source}
\input{db/d79/ustorage__fs_8c}
\input{db/d79/ustorage__fs_8c_source}
\input{d2/dbc/usb__template_8c}
\input{d2/dbc/usb__template_8c_source}
\input{db/daf/usb__template_8h}
\input{db/daf/usb__template_8h_source}
\input{d7/db1/usb__template__audio_8c}
\input{d7/db1/usb__template__audio_8c_source}
\input{d2/d7e/usb__template__cdce_8c}
\input{d2/d7e/usb__template__cdce_8c_source}
\input{d0/d72/usb__template__cdceem_8c}
\input{d0/d72/usb__template__cdceem_8c_source}
\input{d9/d95/usb__template__kbd_8c}
\input{d9/d95/usb__template__kbd_8c_source}
\input{d2/d9c/usb__template__midi_8c}
\input{d2/d9c/usb__template__midi_8c_source}
\input{d3/dc8/usb__template__modem_8c}
\input{d3/dc8/usb__template__modem_8c_source}
\input{d1/db2/usb__template__mouse_8c}
\input{d1/db2/usb__template__mouse_8c_source}
\input{d6/dbf/usb__template__msc_8c}
\input{d6/dbf/usb__template__msc_8c_source}
\input{d9/d15/usb__template__mtp_8c}
\input{d9/d15/usb__template__mtp_8c_source}
\input{d6/d94/usb__template__multi_8c}
\input{d6/d94/usb__template__multi_8c_source}
\input{de/d06/usb__template__phone_8c}
\input{de/d06/usb__template__phone_8c_source}
\input{d5/d32/usb__template__serialnet_8c}
\input{d5/d32/usb__template__serialnet_8c_source}
\input{d3/dcd/ufm__ioctl_8h}
\input{d3/dcd/ufm__ioctl_8h_source}
\input{d3/d75/uftdiio_8h}
\input{d3/d75/uftdiio_8h_source}
\input{d7/d9c/uled__ioctl_8h}
\input{d7/d9c/uled__ioctl_8h_source}
\input{dc/de4/usb_8h}
\input{dc/de4/usb_8h_source}
\input{d1/d1f/usb__bus_8h}
\input{d1/d1f/usb__bus_8h_source}
\input{de/d85/usb__busdma_8c}
\input{de/d85/usb__busdma_8c_source}
\input{da/d02/usb__busdma_8h}
\input{da/d02/usb__busdma_8h_source}
\input{d5/d64/usb__cdc_8h}
\input{d5/d64/usb__cdc_8h_source}
\input{d6/d38/usb__controller_8h}
\input{d6/d38/usb__controller_8h_source}
\input{de/d38/usb__core_8c}
\input{de/d38/usb__core_8c_source}
\input{d2/dd7/usb__core_8h}
\input{d2/dd7/usb__core_8h_source}
\input{dc/da5/usb__debug_8c}
\input{dc/da5/usb__debug_8c_source}
\input{d7/d05/usb__debug_8h}
\input{d7/d05/usb__debug_8h_source}
\input{d7/da4/usb__dev_8c}
\input{d7/da4/usb__dev_8c_source}
\input{db/d48/usb__dev_8h}
\input{db/d48/usb__dev_8h_source}
\input{d4/d42/usb__device_8c}
\input{d4/d42/usb__device_8c_source}
\input{df/db0/usb__device_8h}
\input{df/db0/usb__device_8h_source}
\input{dc/d1b/usb__dynamic_8c}
\input{dc/d1b/usb__dynamic_8c_source}
\input{d1/ddb/usb__dynamic_8h}
\input{d1/ddb/usb__dynamic_8h_source}
\input{de/dc7/usb__endian_8h}
\input{de/dc7/usb__endian_8h_source}
\input{df/d85/usb__error_8c}
\input{df/d85/usb__error_8c_source}
\input{d1/d86/usb__fdt__support_8c}
\input{d1/d86/usb__fdt__support_8c_source}
\input{df/d57/usb__fdt__support_8h}
\input{df/d57/usb__fdt__support_8h_source}
\input{d2/d66/usb__freebsd_8h}
\input{d2/d66/usb__freebsd_8h_source}
\input{d3/d41/usb__freebsd__loader_8h}
\input{d3/d41/usb__freebsd__loader_8h_source}
\input{d9/d58/usb__generic_8c}
\input{d9/d58/usb__generic_8c_source}
\input{db/dae/usb__generic_8h}
\input{db/dae/usb__generic_8h_source}
\input{dd/d42/usb__handle__request_8c}
\input{dd/d42/usb__handle__request_8c_source}
\input{d2/df4/usb__hid_8c}
\input{d2/df4/usb__hid_8c_source}
\input{df/d78/usb__hub_8c}
\input{df/d78/usb__hub_8c_source}
\input{d8/d5d/usb__hub_8h}
\input{d8/d5d/usb__hub_8h_source}
\input{da/d0a/usb__hub__acpi_8c}
\input{da/d0a/usb__hub__acpi_8c_source}
\input{d6/dfc/usb__hub__private_8h}
\input{d6/dfc/usb__hub__private_8h_source}
\input{dc/d18/usb__if_8m}
\input{dc/d18/usb__if_8m_source}
\input{d2/de8/usb__ioctl_8h}
\input{d2/de8/usb__ioctl_8h_source}
\input{db/d60/usb__lookup_8c}
\input{db/d60/usb__lookup_8c_source}
\input{da/def/usb__mbuf_8c}
\input{da/def/usb__mbuf_8c_source}
\input{db/d0c/usb__mbuf_8h}
\input{db/d0c/usb__mbuf_8h_source}
\input{d6/d41/usb__msctest_8c}
\input{d6/d41/usb__msctest_8c_source}
\input{de/df0/usb__msctest_8h}
\input{de/df0/usb__msctest_8h_source}
\input{dc/d52/usb__parse_8c}
\input{dc/d52/usb__parse_8c_source}
\input{d1/d5b/usb__pci_8h}
\input{d1/d5b/usb__pci_8h_source}
\input{dc/d61/usb__pf_8c}
\input{dc/d61/usb__pf_8c_source}
\input{df/d38/usb__pf_8h}
\input{df/d38/usb__pf_8h_source}
\input{d3/d86/usb__process_8c}
\input{d3/d86/usb__process_8c_source}
\input{d4/d25/usb__process_8h}
\input{d4/d25/usb__process_8h_source}
\input{d7/dfb/usb__request_8c}
\input{d7/dfb/usb__request_8c_source}
\input{d8/d00/usb__request_8h}
\input{d8/d00/usb__request_8h_source}
\input{d6/d6f/usb__transfer_8c}
\input{d6/d6f/usb__transfer_8c_source}
\input{dd/d31/usb__transfer_8h}
\input{dd/d31/usb__transfer_8h_source}
\input{dd/db3/usb__util_8c}
\input{dd/db3/usb__util_8c_source}
\input{d9/d69/usb__util_8h}
\input{d9/d69/usb__util_8h_source}
\input{dd/de5/usbdi_8h}
\input{dd/de5/usbdi_8h_source}
\input{d9/df9/usbdi__util_8h}
\input{d9/df9/usbdi__util_8h_source}
\input{d6/d8b/usbhid_8h}
\input{d6/d8b/usbhid_8h_source}
\input{d2/de7/udl_8c}
\input{d2/de7/udl_8c_source}
\input{df/de9/udl_8h}
\input{df/de9/udl_8h_source}
\input{dd/d20/if__rsu_8c}
\input{dd/d20/if__rsu_8c_source}
\input{d7/d84/if__rsureg_8h}
\input{d7/d84/if__rsureg_8h_source}
\input{d3/d1b/if__rum_8c}
\input{d3/d1b/if__rum_8c_source}
\input{de/d86/if__rumfw_8h}
\input{de/d86/if__rumfw_8h_source}
\input{db/dd6/if__rumreg_8h}
\input{db/dd6/if__rumreg_8h_source}
\input{de/ddc/if__rumvar_8h}
\input{de/ddc/if__rumvar_8h_source}
\input{d9/de8/if__run_8c}
\input{d9/de8/if__run_8c_source}
\input{d7/d60/if__runreg_8h}
\input{d7/d60/if__runreg_8h_source}
\input{d6/d2d/if__runvar_8h}
\input{d6/d2d/if__runvar_8h_source}
\input{dc/d94/if__uath_8c}
\input{dc/d94/if__uath_8c_source}
\input{d0/d4b/if__uathreg_8h}
\input{d0/d4b/if__uathreg_8h_source}
\input{d9/d14/if__uathvar_8h}
\input{d9/d14/if__uathvar_8h_source}
\input{d7/de3/if__upgt_8c}
\input{d7/de3/if__upgt_8c_source}
\input{d9/de4/if__upgtvar_8h}
\input{d9/de4/if__upgtvar_8h_source}
\input{db/d79/if__ural_8c}
\input{db/d79/if__ural_8c_source}
\input{da/d30/if__uralreg_8h}
\input{da/d30/if__uralreg_8h_source}
\input{db/d8e/if__uralvar_8h}
\input{db/d8e/if__uralvar_8h_source}
\input{de/d5e/if__urtw_8c}
\input{de/d5e/if__urtw_8c_source}
\input{d4/def/if__urtwreg_8h}
\input{d4/def/if__urtwreg_8h_source}
\input{d2/d69/if__urtwvar_8h}
\input{d2/d69/if__urtwvar_8h_source}
\input{d7/d97/if__zyd_8c}
\input{d7/d97/if__zyd_8c_source}
\input{d4/d2d/if__zydfw_8h}
\input{d4/d2d/if__zydfw_8h_source}
\input{dc/d24/if__zydreg_8h}
\input{dc/d24/if__zydreg_8h_source}
\input{d7/d63/notreviewed_8dox}
%--- End generated contents ---
% Index
  \backmatter
  \newpage
  \phantomsection
  \clearemptydoublepage
  \addcontentsline{toc}{chapter}{\indexname}
  \printindex
% Required for some languages (in combination with latexdocumentpre from the header)
\end{document}
